CPUC Comments on SWWP002-02 VFD on Ag Pump

Lead PA: PGE

Workpaper Plan Submittal Date: 6/18/2021

CPUC Review Date: 07/01/2021

Please note responses to comments in the table below, revise workpaper, and upload the entire package to the WPA. If needed, please reach out to Workpaper Review Team to set up a call to discuss.

|  |  |
| --- | --- |
| CPUC Comment | PA Response |
| Please clarify whether or not the baseline cost source includes throttle valve controls. | The baseline cost includes the cost of the soft starter only; throttle flow control is commonly done using a manual valve, same valve needed to isolate the pumping system, therefore, no additional cost should be added to the baseline. |
| Perhaps if annual operating hours are updated for the enhanced ag pump VFD measure then the same could be done at this time for the tier 1 measure. | This makes sense, adjusting both measures operating hours will reduce the cost and efforts required to perform this update. |
|  |  |