CPUC Comments on SWWH012-02: Storage Water Heater, Residential

Lead PA: SCG

Workpaper Submittal Date: 06/15/2020

CPUC Review Date: 07/01/2020

|  |  |
| --- | --- |
| CPUC Comment | PA Response |
| The measure includes NR, NC, and AR application types. RUL is not required for NR and NC but should be listed for AR measures. Please include RUL, or remove AR offering from the workpaper if no longer applicable. | RUL has been added into the workpaper and RUL ID added into the EAD Tables for AR measures |
| Could not find matching measure codes and savings for all measure offerings in the DEER Water Heater Calculator v4.1.  Measure codes and savings are absent from the calculator for the: 40 gal UEF=0.83; 50 gal UEF=0.88 measures.  Measure savings are absent from the calculator for the 30 gal UEF=0.68 measure. | The edited water heater calculator with the 3 missing measures will be included in the workpaper package.  New TechIDs were created in the calculator for two condensing types (40 gal UEF=0.83; 50 gal UEF=0.88) using the binning file for UEF and capacity.  The 30 gal UEF=0.68 (high draw) tech is already in the calculator, and a measure was created in the calculator using the existing technologies. |

Please note responses to comments in the table below, revise workpaper, and upload the entire package to the WPA. If needed, please reach out to Deemed Review Team to set up a call to discuss.