SDG&E Workpaper Upload

January 2, 2018

Subject: README FIRST File for *WPA Upload of January 2, 2018*

For clarity, this file is included along with the workpaper upload for January 2, 2018 to clarify what information is being uploaded and how SDG&E intends for CPUC Staff to use.

Overall, there are two aspects of this submission:

1. **Update to SDG&E Workpaper “WPSDGEREWH1012\_Rev2\_SF\_Faucet Aerators for Bathroom and Kitchen Sinks in Residential Buildings\_FINAL\_20171228.docx”**: This short form workpaper documents the energy impacts and costs adopted from SCE’s workpaper entitled “Faucet Aerator and Low Flow Showerhead” (SCE17WP004.0 Faucet Aerator and Low Flow Showerhead\_Final.docx). SDG&E adopts all the values in SCE17WP004.0 Faucet Aerator and Low Flow Showerhead, with the following exceptions:
   1. Kitchen faucet aerators are included in this workpaper with a measure case flow of 1.5 gpm.
   2. The SCE workpaper values were adjusted for SDG&E territory. Since SDG&E provides gas and electric the savings use the savings defined as “both” in the Energy Division disposition
   3. Low flow showerheads are covered in a separate workpaper (WPSDGERWH1061A, Rev 5).
2. **SDG&E Ex-Ante data base file “EAD\_2018-01-02\_PUREWP.mdb”:** Ex ante tables for Residential Faucet Aerators included with various other workpaper submittals for January 2nd upload.

Should there be any questions associated with the above, please contact SDG&E Engineering.